Tab. 1: Standard values for ES calculation

|  |  |  |
| --- | --- | --- |
| PM10 | PM10 Buffer Distance | 25 meters |
| Retention | Precipitation | 100 mm |
| Cooling | Period of Heatwave | 1 days |
| Relative Water Content | 0,4 |
| Month of Heatwave | July (7) |
| ET0\_nd | 5,0 |
| Mean maximal Temperature | 26,1 °C |
| Max. Kc value | Max. Kc Value in your AOI (sample data set: 1,3) |